# Partlist

## PCB Layout B2

Partlist exported from C:/code/mp3v2/pcb/RevB2/mp3v2.sch at 10.11.2001 16:40:20

Qty | Value | Parts | Order Code
--- | --- | --- | ---
1 |  | SW1 | Reichelt, PHAP 3301B
1 |  | OUT | Reichelt, PS25/3G
1 |  | PWR | Reichelt, PS25/3G
1 |  | JTAG | Reichelt, PS25/8G
1 |  | LCD | Conrad, #187399
1 | 1M | R9 | Reichelt, 1/4W 1M
2 | 1k | R10, R14 | Reichelt, 1/4W 1K
1 | 4k7 | R2 | Reichelt, 1/4W 4.7K
1 | 5k6 | R6 | Reichelt, 1/4W 5.6K
1 | 10µ | C10 | Reichelt, rad 10/25
1 | 10µ | L1 | Reichelt, SMCC 10µ
2 | 10k | R5, R13 | Reichelt, 1/4W 10K
1 | 10n | C5 | Reichelt, Z5U-2.5 10n
1 | 12.288 MHz or 24.576 MHz | Q1 | Reichelt 12,288-HC18 or Segor, Q 24,576-GW
2 | 15R | R11, R12 | Reichelt, 1/4W 15R
2 | 33p | C8, C9 | Reichelt, Kerko 33p
2 | 47R | R3, R4 | Reichelt, 1/4W 47R
1 | 74LS245DW | IC6 | Reichelt, SMD LS 245
2 | 100µ | C13, C14 | Reichelt, SM100/16rad
9 | 100n | C1, C2, C3, C4, C6, C11, C12, C15, C17 | Reichelt, Z5U-2.5 100n
1 | 150R | R1 | Reichelt, 1/4W 150R
1 | 180R | R16 | Reichelt, 1/4W 180R
1 | 210R | R8 | Reichelt, 1/4W 210R
2 | 220µ | C7, C16 | Reichelt, rad 220/16
2 | 330R | R7, R15 | Reichelt, 1/4W 330R
1 | BC547C | T1 | Reichelt, BC 547B
1 | BLUE | D2 | Reichelt, LED 3mm ST-blau
2 | GREEN | D1, D3 | Reichelt, LED 3mm ST-grün
1 | HALO | HALO | Beck, Ethernet Transformer
1 | IDE2.5 | IDE2 | Conrad, 2x #739219
1 | IDE3.5 | IDE1 | Reichelt, WSL40G
1 | JACK8SH | ETH | Reichelt, MEBP 8-8G
1 | LM317LZ | IC5 | Reichelt, LM317 TO92
1 | PG203J | X2 | Reichelt, EBS 35
1 | SC12 | IC2 | Beck, IPC@Chip SC12
1 | TL 7705 | IC1 | Reichelt, TL 7705 DIP
1 | TSOP1738 | IC4 | Reichelt, TSOP 1738
1 | VS1001SOIC28 | IC7 | Segor, VS 1001k
1 | ispLSI1016 | IC3 | Reichelt, ispLSI 1016-LJ

## Recommended Components

- You definetely want 0.5mm solder, and desoldering-wick to assemble the PCB.
- Soldering IC3 is much easier, if you use a SMD PLCC socket, Break out the inner plastic part of the socket before soldering.
  - Reichelt, SMD PLCC 44
- You'll need a 26pin cable and connector, if you want to use the graphic LCD.
  - Reichelt, PFL 26
  - Reichelt, 1m AWG 28-26G
- Don't forget to buy small distance nuts, if you want to mount a 2.5" HD directly on/under the PCB.
  - 4x Reichelt, DA 10mm
- You might want to buy a small 5V switching power supply.
  - Reichelt, PSA 15W-050, (Phihong 15W, 5V)
  - Reichelt, ADC120 (AC Power cord)
  - Reichelt, HEBLM 21

## Where to get the parts?

All parts can be ordered through the online shops of Reichelt, Segor, Conrad, and Beck automation.

- www.segor.de
- www.reichelt.de
- www.conrad.de
- www.bcl-online.de
- 2.5" Harddisk cables www.kabelspezialist.de

Please mail me, if some parts are not available, or you have problems with your order.